	TAIVA

Nauticat 331

· Year: 1999 

· Current Price: € 180000 

· Hull Material: Fiberglass 

· Engine/Fuel Type: Single Diesel 

YANMAR 88HP

Description
NAUTICAT 331 built by Sitala Yachts in Finland to designs by Kaj Gustafsson
Commissioned in May 1999.

CONSTRUCTION:

White GRP hull and superstructure with teak seating, side decks and fore-deck.
Fin keel.  Dual steering station - Capilano Hydraulic system.  Interior joinery is rubbed effect varnished teak with teak and holly cabin sole throughout.

All exterior trim, including handrails, are of teak.
All windows of toughened safety glass suspended in alloy frames.
Stainless steel stanchions with teak rails.
Four heavy duty mooring cleats and four heavy-duty fairleads.
Extra cleats positioned midships on port and starboard.
TWO Stainless steel heavy-duty dual anchor roller stemhead fitting.
Teak caprail.
Anchor locker on fore deck.
Varnished teak 50 cm steering wheel in pilothouse.
Stainless steel Strazo 80 cm steering wheel on deck with elk hide cover.
Emergency steering tiller mounts direct to rudder stock.

LOA: 11.4m 

LOD: 10.4 m 
LWL: 8.6m 
Beam: 3.4m 

Draft: 1.65m (deep lead keel)
Displacement: approx 8.3 tons (17,000lbs)




	
Inventory


NAVIGATION AIDS:
Suunto 6" No 136 magnetic compass in Pilothouse.

Hinged magnetic compass aft deck.

Navigation equipment for chart work.


WHEELHOUSE

Raymarine RL70C colour LCD plotter/radar with 2kw scanner on mizzen mast.
Panasonic C72 ruggedised computer with Maxsea charts for Europe from U.K. to Mediterranean.
Firdell Blipper radar reflector.
Leica GPS linked to chart, radar, and VHF radio.

Secondary Furono GPS linked to all instruments with cross over switch. 
Raymarine ST60 wind speed and direction (2008).
Raymarine electronic compass.

Raymarine Trim instrument.

Raymarine Masterview instrument.

Raymarine Multiview instrument.
Raymarine ST6000+ hydraulic autopilot with repeater at second helm.
Simrad RD68W DCS VHF radio.

Handheld waterproof Simrad VHF

SSB radio.

Navtex

Fax 4 weather receiver.

Digital ammeter/voltmeter.

Solar panel ammeter.

Built in printer

Bow thruster control.

Electric switches for anchor control.

AFT DECK.

Raymarine ST6000+ hydraulic autopilot

Raymarine ST80 wind speed and direction

Raymarine Trim instrument.

Raymarine Masterview instrument.

Raymarine Multiview instrument.

Electric switches for anchor control.

Bow thruster control.

12V socket

Electric socket for dinghy pump.

Mechanical bilge pump.

Two waterproof speakers connected to sound system. 


GROUND TACKLE:
23Kg (51 lb) CQR stock anchor with 60m (180 ft) chain warp.
12Kg (26 lb) Fortress anchor with 5m chain, two 50m (164 ft) polypropylene warps.

200M spare warps.

12Kg Kedge anchor with chain and tape mounted on stainless steel wheel.
Lofrans electric windlass.
 Anchor box in fordeck with overboard drain.

Electric foot controls for anchor.

Connector for hand held anchor control. 


GENERAL EQUIPMENT:
Six fenders.

Two large inflatable Avon fenders.

Two horseshoe lifebuoys with holders.
Opening gates in lift lines on both sides.
Electric stainless steel horn mounted at mast, with switch at helm.
Three windscreen wipers with independent switches.
Four 15m (45 ft) braided warps.

Two 25mm 10M warps with chains for marina.
Propane tank in separate deck locker with overboard drain and shutoff valves.
Dual electric bilge pumps.
Henderson manual bilge pump.
Black and Decker cordless drill.

SAFETY EQUIPMENT:
Six man cannister liferaft with cradle.
Two lifebuoys (one with strobe light)
RORC flare pack .
Six  lifejackets.

Six double clasp life-lines.

Port and Starboard Jackstays.

Navigation lights including steaming and anchor lights to international rules.
Deck flood lights on main and mizzen masts.
Search light.

Lee cloths to all bunks
2 Kg fire extinguisher
6 Kg fire extinguisher.
1 Fire blanket.

	


	
Machinery


YANMAR 88 HP 4 CYL TURBO DIESEL:
Full engine service August 2008.
1650 hours on 5 September 2008.
Fresh water cooling with heat exchangers.
Shaft drive, bronze bushings with lubrication system.
Maxprop three bladed propeller.
Dual engine controls.
Electric push button engine oil change system.
Cruising range approx 600 nautical miles.
4 HP Sliepner bow thruster with cockpit joystick.
Fuel gauges, battery charge level, tachometer, oil pressure, temperature, ampere meter, engine hours and holding tank level.

ELECTRICS:
THREE x 12v 180 AH house batteries Pavillion (2008)
12v 135 AH engine start battery Exide HD.
12v aux bow thruster battery.
Mastervolt 40 amp Smart Charger plus solar battery charging panels.
240v shore power with 25m dock cable.
12v power points at both helm stations for mobile phones etc.

Power points and 12v sockets in all areas.

Graphite grounding connector on engine shaft.

TANKAGE:

Fuel capacity: 600 litres in two 300 litre tanks each side of the engine room, vented with side deck fills. Tanks have separate manual pump for clean out of sludge.
Fresh water capacity: approx 600 litres in a polyethylene tank beneath the cabin sole.
Water tank fills from deck and has a large tank inspection clean out port.

Water filter in Galley.
Separate stainless steel fresh water tank supplies toilet for flushing.
Holding tank capacity: approx 80 litres.


WATER SYSTEM:

Pressurised hot and cold water system with filter to galley.

Calorifier with immersion / engine hot water.

HEATING:

Eberspacher heater provides ducted hot air throughout boat and lockers.



	


	
Rigging


KETCH RIG:

Selden anodised aluminium spars.

In mast main.

Removeable forestay (Highfield lever) and staysail.

Internal halyards (disassembled and inspected November 2004).

Spare main and forestay.
Genoa with Furlex roller reefing.
Rodkick boomvang.
Spinaker pole with inbuild halyards.
Flag halyards at spreaders and mainmast.
Two Harken 2 speed self tailing genoa winches.
Two 8" and two 10" winch handles.

SAILS: by North Sails.

Genoa with UV strip.
Mainsail.

Genaker with snuffer (new)

Staysail (new)
Mizzen with lazyjacks.


	

	Accommodation


SIX BERTHS IN THREE CABINS:
 6'+ headroom.  Metal mosquito nets.
Reflective blinds to main hatches.

PILOTHOUSE:
U shaped royal blue heavy cotton twill upholstered seating (complete new covering material also available), custom dining table. Additional extra collapsible table for aft deck. Inside helm station with specially designed layout for instrumentation, ample locker space and chart storage. Furnished with curtains and insect screens on all port lights and hatches. Overhead and reading lights.  Attractive floor carpets throughout (two new sets unused).  Built in television and radio with four speakers.
Brass clock, barometer and hygrometer.  Behind starboard steps many tools and spares, oil and cleaning equipment.  Lower locker behind table, tools, flares, warps, storage containers, spare anodes.

Lower starboard locker inverter for T.V. and using mains equipment away from shore power.  Manual and electric pumps for Avon 2.9m dinghy.

Storage either side of helm, navigating instruments and more small general equipment.

Extra room for charts in locker under T.V. 


AFT CABIN:

Large aft cabin with two large single bunks. Lockers, drawers and storage space with two bookshelves. Lighting consists of downlights and reading lights. Pillows, duvets and fitted sheets.


FORWARD CABIN:

Two single berths in a V configuration with extra thick foam mattresses. Lockers, storage space and bookshelves. Lighting consists of downlights and reading lights. 

Large mirror.  Duvets, pillows and fitted sheets.  Dehumidifier, warps, bucket, electric drill, etc, stored beneath bunks. 

GALLEY:

Two burner Tropic gimballed propane gas stove with oven.  Top opening 12v fridge. Stainless steel sink. retractable chopping board and work counters over appliances. Deck hatch over cooking area for excellent extraction with 12v extractor fan.  Glasses and special mug rack.  Plates, bowls, knives, forks and spoons, pans and all general kitchen equipment.

SALOON:

U shaped seating in matching material to wheelhouse around large table that converts to spacious double bed.  Separate drinks cabinet and glasses cabinet.  Large storage areas under seating.

HEADS:

Ceramic toilet bowl with secure hand pump operation.  Ceramic washbasin with hand shower.  Dorade ventilation.


 DECK:

Stainless steel handrails on cabin tops. Anchor locker with drain. Electric anchor windlass with three remote controls. Canvas covers for windlass, winches, and aft steering wheel. Dorade deck ventillators to cabin. Sprayguards provided for pilothouse doors. Backrest cushions for mounting on handrails in aft cockpit. Attractive stainless steel steps mounted at stern. 

	

	Broker Comments
This is an exceptional example of the Nauticat 331. Built to a very high specification, with considerable thought put into every aspect of the design. Taiva comes with a wealth of navigation equipment and recently fitted batteries and new wind instrument installation.  Sail anywhere in comfort and style. 

	


