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	Description:

	At 50 knots, the confidence and power of this craft is simply awe-inspiring. Performance levels can be adjusted depending on your preference of engine and drive systems. Accommodation is as generous as it is comfortable, whilst an immense upper-deck saloon is fitted with a stylish bar and day galley. On deck, ample sunbathing space and a retractable bimini top over a huge cockpit area make for effortless entertainment.

	 

	Specifications:

	Vessel Type:
	Sports Yacht
	Designer:
	Sunseeker

	Builder: 
	Sunseeker 
	Model: 
	Predator 100 

	Length (LOA):
	29.81 m 
	Draft ;
	6.32 m

	Beam:
	6.32 m 

	Propulsion: Direct gear drive through triple Arneson surface drives.
Engine option:
3 x MTU 2000 V16 2029PS (1492kW/2000bhp)
Top speed: up to 49 knots
Range: up to 400 miles (subject to speed)

ENGINE ROOM:

Separate fuel filters for each engine with water sensors
Fuel filter for each generator
Fuel tank with electric sender unit
Manual bilge pump with changeover valve to pump fore and aft 
Bilge pumps (24v automatic) engine room = 1 x flood pump 3700 litres/hr and 1 x 1500 litres/hr pump
Amidships = 1 x flood pump 3700 litres/hr and 2 x 1500 litres/hr pump

Bilge water flood alarm forward and aft

Electric 24v scavenger bilge pump in engine room
Sound insulation throughout engine room
Fresh-water engine top up hose and spigot
24v lead light

Automatic FM200 fire extinguishing system with engine/generator and fan shut down 
24v hydraulic pump for trim tabs, platform and garage door
24v hydraulic pump for gangway
Gearbox driven hydraulic pump for bow and stern thruster
Telephone point
Fuel shut-off valves operable from inside and outside engine room
Watertight forward and aft engine room bulkheads

SYSTEMS
24v hydraulic pump for trim tabs, gangway and garage door
Hydraulic power steering from engine driven pump
Tecma toilets (24v) with 1 switch control (incorporating tank level indicator)
Toilets discharging overboard or to black water tank
Black waste water-tank discharging to deckside or overboard through (24v) macerator pump
Fresh water-tank with sending unit
AC fresh-water pressure system 
24v DC back-up fresh-water system
Watermaker (2387 litres per day/630 US gals per day) 
Hot water cylinder with AC immersion heaters
Chilled water air conditioning system (reverse cycle)

ELECTRICAL SYSTEM
Glendinning cable master dockside connection (1 x 100ft lead with remote and 1 x 50 amp shorepower socket)
Television and telephone dockside connection
Galvanic isolators
Main DC and AC breaker panel/circuits protected by re-settable circuit breakers
Systems monitoring panel
Change-over protection for generators
Remote battery switches controlled from locker in aft cockpit
2 x 95 amp battery chargers 24v
1 x 80 amp combi/charger
1 x 40 amp battery charger 12v
Battery coupling system
Alternators on engines and generators
Battery bank for engine starting 24v
Battery bank for domestic power 24v
Battery bank for 12v items
2 x 2kW immersion heaters 
AC outlet sockets throughout the boat
Engine bay and bilge lights
Engine room extractor fans
Television antenna and circuit Glomex

GENERATORS
Europe: 2 x 23kW @ 50Hz generators with sound shield
US: 2 x 28kW @ 60Hz generators with sound shield
Water separator/silencer on generators
12v starting for generators
Remote starting

UNDERWATER GEAR
Direct V drive through tunnels
Stainless steel temet propeller shafts
High performance bronze rudders and struts
Bronze P-brackets
Dripless shaft logs

	No. of Engines:
	3

	Fuel type:
	Diesel

	Drive type:
	Surface piercer

	Construction: 

	GENERAL CONSTRUCTION

Built to comply with RINA 100 A1 Classification (not certified) 


Built to European specification 220v single phase 50Hz
or
Built to USCG Regulations 220v/110v single phase 60Hz

Hull and deck
Gel coat including stripes
Vinyester skin coat with powder bound mat
Stitched multi-axial single skin hull bottom
Balsa/PVC foam cored topsides – skinned with stitched multi-axials
PVC foam cored deck
Longitudinally stiffened with foam formers over-laminated with stitched multi-axials
Transversely stiffened with GRP ringframes, marine ply and sandwich bulkheads

Superstructure
Gel coat
PVC foam cored and skinned with stitched multi-axials
Stiffened with foam formers over-laminated with stitched multi-axials

	Hull Material:
	Glass Fibre

	Hull type:
	Deep V

	Accommodation:

	DECK SALOON
Opening hardtop roof
Teak-laid saloon floor
Access stairs forward to lower deck
Dining to starboard side
Casual seating to port
Storage cabinets with glassware for 8 and bottle stowage
Wine cooler
Scatter cushions
LCD flatscreen TV (42") on rise and fall
Nicam stereo VCR
CD/DVD/Radio surround-sound system 
Magic eye for control of entertainment systems
Sideboard area
Sliding curved glass patio doors opening to aft cockpit 
Side windows with electric blinds
Halogen overhead lighting 24v
Telephone point
AC double sockets
Air conditioning 
Hand-held fire extinguisher

LOWER SALOON AND LOBBY
Staircase from deck saloon
Access to accommodation cabins
Lounge seating with low table

LCD flatscreen television (42")
CD/DVD/Radio surround-sound system
Nicam stereo VCR
Magic eye for control of entertainment systems
Halogen overhead lighting 24v
Table lamps (subject to layout)
AC double sockets
Large fixed tempered glass portholes with blinds
Air conditioning 
Telephone point
Drinks cabinet
Hand-held fire extinguisher
Fitted carpet

GALLEY
American style fridge/freezer with ice maker
4-ring ceramic electric hob
Electric oven
Coffee machine (free standing)
Microwave
Dishwasher (slimline)
Rubbish bin

Extractor fan
Sink and drainer (stainless steel) with beech insets
Waste disposal unit in sink
Granite worktop
Planked wood flooring
Halogen overhead lighting 24v
AC double sockets
8 place settings crockery and cutlery
First aid kit
Hand-held fire extinguisher
Large fixed tempered glass portholes with Venetian blinds
Air conditioning

OWNER’S STATEROOM
Double berth with sprung mattress
Bedcover, sheets and pillowcases
Bedside tables
Bedside lights
LCD flatscreen television (19")
CD/DVD/Radio surround-sound speaker system 
Magic eye for control of entertainment systems
Opening tempered glass portholes with blinds
Halogen lighting 24v
Wardrobe with light
Storage
Safe deposit box
Air conditioning
AC double sockets
Telephone point
Hand-held fire extinguisher
Dressing table with stool
Door to en suite

OWNER’S STATEROOM EN SUITE
Tecma toilet 24v
Bidet
Granite vanitory top
Granite floor
Washbasins
Shower cubicle
Taps and accessories
Mirror
Extractor fan
Opening tempered glass porthole with Venetian blind
Razor socket
Halogen lighting 24v
Air conditioning outlet
Door to stateroom

FORWARD VIP STATEROOM
Double berth with sprung mattress
Bedcover, sheets and pillowcases

Halogen lighting 24v
LCD flatscreen television
CD/DVD with four speakers 
Opening tempered glass portholes with curtains
AC double socket
Air conditioning
Telephone point
Hand-held fire extinguisher
Fitted carpet
Dressing table with stool
Wardrobe with light
Emergency escape hatch to foredeck
Door to en suite

VIP EN SUITE
Tecma toilet 24v
Granite vanitory top
Granite floor

Wash basin
Shower cubicle
Taps and accessories
Mirror
Extractor fan
Opening tempered glass porthole with Venetian blind
Razor socket
Halogen overhead lighting 24v
Air conditioning outlet
Door to stateroom

STARBOARD GUEST CABIN
Twin berths with sprung mattresses
Bedcover, sheets and pillowcases
Bedside table
Reading lights
Storage
Halogen overhead lighting 24v
Opening tempered glass porthole with blind
Air conditioning 
LCD flatscreen television
CD/DVD with two speakers
AC double socket
Telephone point
Wardrobe with light
Fitted carpet

PORT GUEST CABIN
Twin berths with sprung mattresses (bunk berth option subject to layout)
Bedcover, sheets and pillowcases
Bedside table
Reading lights
Storage
Halogen overhead lighting 24v
Opening tempered glass porthole with blind
Air conditioning
LCD flatscreen television
CD/DVD with two speakers
AC double socket
Telephone point
Wardrobe with light
Fitted carpet
Door to en suite

GUEST TOILET AND SHOWER ROOM
Tecma toilet 24v
Granite vanitory top
Granite floor
Wash basin
Shower cubicle
Taps and accessories
Mirror
Extractor fan
Opening tempered glass porthole with Venetian blind
Razor socket
Halogen overhead lighting 24v
Air conditioning outlet
Doors to port guest and lobby

CREW CABIN (SUBJECT TO LAYOUT)
Access door from sidedeck and stairs into cabin (subject to layout)
Large single berth with foam mattress
Bedcover, sheets and pillowcases
Halogen overhead lighting 24v
Opening tempered glass porthole with curtains
AC double socket
Air conditioning
Telephone point
Washer/Dryer
LCD flatscreen television
CD/DVD with 2 speakers
15 Crew toilet and shower room

Tecma toilet 24v
Vanitory top
Wash basin
Shower 
Opening portlight with Venetian blind
Taps and accessories
Mirror
Extractor fan
Razor socket
Halogen overhead lighting 24v


	

	Equipment:

	DECK
Teak-laid side decks
Anchor winch and capstan 24v
Chain stop
Bruce anchor 80kg and chain (galvanised 100m)
Automatic chain wash (fresh water) 
Stainless steel bow plate 
Stemhead roller in stainless steel
Twin bow cleats and fairleads in stainless steel
Two pairs of spring cleats and chafing bars in stainless steel
Twin stern cleats and fairleads in stainless steel
Two stern capstan winches 24v
Twin retractable platform cleats in stainless steel
Stainless steel side rails
Fresh-water deck wash with outlets forward and aft
Remote controlled retractable gangway
4 x pantograph wipers and windscreen washers
IMCO navigation lights
Forward sunbathing pad
Cup holders
Forward seating area
Ensign staff/socket
Fender and rope lockers port and starboard
Fuel fillers port and starboard
Fresh-water filler
Port and starboard doors to sidedecks
Sidedeck and foredeck low-level lighting
Remote controlled spotlight on bow
Forward emergency escape hatch (from VIP stateroom)
Fire hydrant located in forward locker

AFT COCKPIT AND BATHING PLATFORM
Cockpit table and seating
Three folding chairs
Casual seating areas
Aft retractable sunbathing pad
Retractable canopy
4 x marine speakers connected to hi-fi in deck saloon
Bar with cool chest, ice maker, sink with hot and cold water and griddle
Low- and high-level lighting
Teak-laid cockpit floor
2 x 8 man liferafts (non SOLAS approved)
Television and telephone dockside connection
Fresh-water dockside connection
Hand-held fire extinguisher
Shorepower connection for AC (1 x 100 amp Glendinning, 1 x 50 amp socket)
Boat hook
Engine room access hatch
Stainless steel safety gates to bathing platform
Large bathing platform (hydraulic rise and fall, tilting only with triple engine option)
Teak-laid steps and bathing platform
Fold-out bathing ladder
Hot and cold swimming shower
Fibreglass radar arch

Airhorn
Loudhailer
Fire hydrant outlet located aft

STERN GARAGE
Hydraulic opening stern garage 
Tender launch and recovery system with winch
Waterproof lighting
AC socket in waterproof enclosure
DC socket in waterproof enclosure

HELM POSITION
Four fully adjustable electric helm seats
VHF radio
Hydraulic power steering
Electronic throttle and gear controls
Radar/Chartplotter with GPS (2 x colour screens)
Autopilot
Depth and speed displays
Magnetic compass
Loudhailer control (via VHF handset)
Remote spotlight control
Bow and stern thruster control
Anchor winch control
Air horn control
Rudder reference gauge (twin engine option) 
Trim tab controls 
Arneson drive controls and indicators (triple engine option)
Monitoring system panel
Full analogue engine instrumentation
Fresh-water gauge
Fuel gauge
Telephone point
Double AC socket
Windscreen demister
Cigar lighter
Halogen overhead lighting 24v
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