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Main characteristic

Name:
Etesian

Type:
Staysail Schooner

Shipyard:
C&B Marine St. Cruz California

Architet/Designer:
 J.G. Alden (on 1936 drawings)

Year:
1983

Hull material:
Wood (Cold molded)

Registry:
Gibraltar

Berth:
La Spezia

Partial refit in 2001

Main refit in 2003

Partial refit in 2006
Dimension

L.O.D:
19.62 mt. / 64’4” plus bowsprit

Beam:
4.70 mt. / 15’5“

Draught:
2.60 mt. / 8’6”
Displacement:
54.27 tons

Max. Speed:
10 knots (under power)

Cruising speed:
7-8 knots (under power)

Range:
Approx. 800 NM

Consumption:
Approx. 10 lt./hour (6 gallons / hour)

Price:
Under request

VAT:
Paid

Flag:
Gibraltar

Rig

Rig:
Steel (replaced in 2003)
Masts:
Aluminium (painted in 2003)
Booms:
Wood
Sails
Mainsail:
Doyle (2001)

Foresails:
1 jib roller furling (2001)


1 set Doyle of  2 staysails, white (2001)


1 assymetrical Doyle staysail, red (2001)

1 fisherman white (2001)


1 gollywobbler multi colour

Whinces 

Cockpit:
1 Barient 28 electric selftailing 2 speed


2 Barient 32 selftailing


2 Lewmar 66 electric selftailing (2003)

Main mast:
2 Barient 28 selftailing


1 Lewmar 40 selftailing

Fore mast:
2 Lewmar 44 selftailing (2001/2003)


1 Lewmar 40 selftailing (2003)


1 Barient 27 selftailing

Deck:
2 Lewmar 48 selftailing (2001)
Machinery

Engines:
Perkins 135 HP / 100 kW (2001)

Tankages

Fuel Tank:
3 x steel, total 900 lt
Fresh water tank:
2 x steel, total 400 lt and 3 x plastic, total 150 (2003)

Waste water tank:
Steel 100 lt (2003)

Electric system
Generator:
Lombardini  8kw @ 1500 rpm (2003)

Votlages:
220 V / 24 V / 12 V

Inverter (V/M):
Mastervolt

Battery Charter:
1x Mastervolt 24/50 plus one spare


1x Mastervolt 12/40 plus one spare

Batteries:
12 V for engines


12 V for generator


24 V services

Shore power:
220 V
ALL THE ELECTRIC SYSTEM HAS BEEN COMPLETELY REDONE IN 2003

Navigation equipment

Autopilot:
Simrad-Robertson J300x40 (2001)

GPS/Plotter:
Simrad CA 50W interior and DS 50 exterior (2001)

Radar:
Simrad CA 50W interior and DS 50 exterior (2001)


Weatherfax:
InmarsatC  Thrane & Thrane TT-30022D (2001)

Navtex:
Yes

Depth sounder:
Simrad CA 50 W interior and DS 50 exterior (2001) + Horizon exterior (2002)

Wind indicator:
Horizon (2002)

Extra:
Handle GPS

Comunication equipment

Telephone:
GSM Panasonic interface with PC (2003)

VHF:
Sailor DSC (2001)
SSB:
Kenwood interface with PC (2003)

Satcom:
MiniM Simrad interface with PC (2003)


Inmarsat C Thrane & Thrane interface with PC (2003)

PC:
Philips Pentium 4 / Icom screen (2004)
Handle FM:
2x ICOM + 2x Motorola

Handle VHF:
2 x ICOM

Entertainment

Saloon:
Panasonic Home Theatre with flat screen TC-22LT1 35”

Paioneer CD 


Paioneer DVD cod 1 (USA)

Owner cabin:
Sony CD 

Guests:
Sony CD 
Crew:
Sony CD
Distribution

Owner Cabin:
2 double berths


1 Closet

2 drawers dresser + 6 drawers on the berth level

1 bathroom with large shower/bath and TECMA electric toilet (plus full spare)
Guests Cabin:
2 single berth


1 closet

1 drawers dresser

1 bathroom with shower and TECMA electric toilet (plus full spare)
Crew Cabin:
2 single berth plus a 1 small

1 bathroom with shower and TECMA electric toilet (plus full spare)

Saloon:
1 table for 6/8 persons

1 large U shape sofa 6/8 persons  convertible into bed


1 large sofa 3 persons convertible into bed

Galley:
Forward to saloon on backboard

Appliances

Refrigerator:
2x Frigorboat W50F (2003)

Deep freezer:
1x Frigorboat W50F (2003)

Microwave:
1x Sharp (2003)

Stove:
electric Force 10 with 3 burners and oven

Water heater:
1 electric 100 lt.
Deck equipment

Gangway:
Carbon fiber

Bathing ladder:
Royal ladder

Deck shower:
1

Awning:
yes

Bimini top:
yes (2001)

Sun Mattresses:
yes (2001)

Covers:
yes (2001)

Protection cover:
yes for skylight, entrances, side hull, wheel, winches (2001/2006)

Anchors:
2 x 60 kg (2004)

Windlass:
2 x Maxwell 3500

Chain:
1 x 60 m. (diameter 14)


1 x 120 m. (diameter 14)

Deck wash system:
yes

Tender and water toys

1 wooden skift 12 ft 

available in Palma de Mallorca 1 avon jet 60 hp to be fixed
Safety

Life raft:
1x 8 persons Eurovinil with hydrostatic relize
Life jackets:
14 x Safe Guard Corp. USCG approved

Epirb:
1x

Sistema antincendio:
Semi automatic FI QUENCH MARK III

Fire extinguisher:
6x Co2 (2001)

Bildge allarm:
yes
Lupo Yacht Services Srl

Sede operativa: Marina di Varazze,  Via Savona, 17019 Varazze (Sv)

Phone: +39 019 939 9248 / +39 019 935 888 -  Fax: +39 019 935 3546 - Mobile: +39 348 396 4544

Sede legale:  via Repubblica 65,  28053 Castelletto Ticino (No)

Web: www.lupoyachtservices.com - email: info@lupoyachtservices.com
P.IVA 02039360033
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