PRINCESS 54

TECHNICAL SPECIFICATIONS
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PRINCES 54 - ELEGANT AND EXQUISITELY FINISHED, THE BENCHMARK FOR HER CLASS  Seated on the flybridge of the Princess 54, cruising through open water in supreme comfort, it is hard to imagine a more perfectly proportioned motor yacht. Her form is definitively Princess with a deep V hull, dynamic deck lines and expansive windows that combine in a stunning profile and afford panoramic views from within the light, airy main deck.  The imaginative layout provides a variety of locations in which to relax; the expansive flybridge with double sunbed, convivial U-shaped seating and wetbar, plus the large cockpit and welcoming open plan saloon. Here, there is ample room to relax in the comfort of the U-shaped sofa, or to take in the views from the raised dinette. A cocktail bar and the beautifully finished and fully-equipped galley below provide the essentials for relaxed entertaining on board.  Below decks, the accommodation includes three large cabins plus an optional crew cabin aft. The owner's stateroom, extending across the full beam, features vertical portholes on both sides as well as an en-suite bathroom with separate shower. The forward stateroom, sumptuously upholstered, also has an en-suite, while the generous twin berth cabin features side-by-side bunks and provides full standing headroom.  Elegant and exquisitely finished, the 54 is widely recognised as the benchmark for her size range.
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PRINCIPAL DIMENSIONS Length overall (incl. pulpit) 54ft 5in (16.57m) Length overall (excl. pulpit) 53ft 5in (16.26m) Beam 15ft (4.57m) Draft 4ft 2in (1.27m) Displacement approx. (Twin Volvo D12-800) 23,500 kgs* (51,808lbs) Fuel capacity 550 gal/660 US gal/2500l Water capacity (incl. calorifier) 130 gal/156 US gal/592l  

STANDARD EQUIPMENT Power-assisted hydraulic steering system Bow thruster (125kgf/276lbf) 24v DC/240v AC electrical system 240v shore power with 80-amp float battery charger 220v/240v diesel generator (9.5kW) Dual station remote control electric anchor winch Dual station electric trim tabs with indicators Dual station autopilot Dual station VHF with DSC R/T with intercom Dual station speed and distance log Dual station echo sounder with alarm Remote control searchlight Combination microwave/conventional oven/grill Full height refrigerator/deep freeze Cocktail cabinet with refrigerator Flybridge wetbar including sink and electric barbecue Flybridge top loading coolbox Flybridge sunbed and cushions Electric quietflush toilets Saloon LCD TV/DVD/radio linked to flybridge speakers Stereo CD/radio in owner’s stateroom Teak-laid transom platform/cockpit deck/flybridge stairway/stairs to side decks Triple opening stainless-steel framed saloon doors Full length transom platform with tender storage facilities Transom door Hot and cold transom shower Cockpit night covers  

ENGINES – DIESEL Twin Volvo D12-800 (2 x 775mhp) Speed range: 31-34 knots  

DECK FITTINGS Teak-laid transom platform, cockpit deck, flybridge stairway and stairs to side decks Reversible electric anchor winch with foredeck, main helm and flybridge controls Self stowing 25kg Delta anchor with 40m of chain Stemhead roller with automatic anchor launch and retrieve Stainless steel bow, stern and spring cleats Stainless steel bow fairleads Stainless steel pulpit and guard rails with fender baskets Stainless steel coachroof and flybridge rails Stainless steel rubbing band with rubber insert Full set of IMCO navigation lights Riding light Twin beam searchlight with dual-station remote controls Twin electric horns Fuel and water fillers

  AFT COCKPIT Self-draining Upholstered seat Hatch on gas strut to lazarette storage Lockable access hatch to engine room Steps to side decks Cockpit lighting Transom gate leading to bathing platform Side lockers Fender storage 220/240v shore support inlet Stainless steel handrails Remote fuel cocks located in locker Access to engine room Integral stairway to flybridge with teak treads Transom teak laid bathing platform with foldaway swimming ladder, hot and cold shower Transom storage locker Dinghy chock system

  FLYBRIDGE Dual station instrument controls (see Lower Helm Position) Visible and audible engine warning system Bilge pump audible alarm Double helm seat U-shaped seating for 6 with table Separate sunbed aft with storage below Wetbar with sink and electric barbecue Refrigerated coolbox Loudspeakers linked to saloon stereo Integral stairway from aft cockpit with perspex hatch Wind deflector screen Stainless steel handrails GRP radar arch Console and seat covers Matched whip aerials for VHF R/T and radio  LOWER 

HELM POSITION Twin helm seats with fore and aft adjustment for helmsman Opening side window Burr elm instrument console with engine instruments and fuel gauges Dual station instruments and controls at Flybridge and Lower Helm Position: - rudder position indicator - electronic engine controls - power-assisted hydraulic steering - bow thruster controls - anchor winch remote control - trim tab controls - autopilot - VHF DSC R/T - speed and distance log - echo sounder with alarm - searchlight remote control - high-speed magnetic compass - horn button Navigation light switches Flybridge intercom, loudhailer and foghorn Chart table with light and chart stowage Windscreen wipers with freshwater windscreen wash system Bilge pump controls with visual ‘pump running’ warnings 24v and 240v electrical control panels PVC sunscreens 24v and 240v control panel

 

DECK SALOON
U-shaped sofa with table starboard side Port sideboard unit Bottle and glass storage Refrigerator LCD TV/DVD/radio with saloon and exterior speakers Triple stainless steel framed sliding doors Tinted windows Curtains or sunscreens to all windows and doors Overhead downlighters Clock and barometer

 

GALLEY Avonite (or similar) worktop 4-zone ceramic hob Combination microwave/ conventional oven with grill Stainless steel sink with mixer tap Chopping board Full height fridge (199 litres)/ freezer (71 litres) Waste disposal bin Overhead and concealed lighting Drawers and storage cupboards Dedicated cutlery drawer Provision for washer/dryer (opposite)

 

ACCOMMODATION All cabins and bathrooms feature opening and/or fixed portholes and electric quietflush toilets (except for optional crew cabin where marine WC features)

  OWNER’S STATEROOM Large double bed Twin bedside tables Wardrobe and shelves Dressing table Mirror Storage lockers and drawers Downlighters and individual berth lights Stereo CD/radio  En-suite shower/WC: Washbasin with Avonite worktop Mirror Toothbrush/mug and towel holders Shower compartment with automatic pump out Extractor fan

  FORWARD STATEROOM Large double bed Wardrobes and shelves Storage lockers and drawers Mirror Dressing table with mirror Downlighters and individual berth lights Deck hatch with flyscreen and blind Stowage location for dinette stools (2)  En-suite shower/WC: Washbasin with Avonite worktop Shower compartment with automatic pump out Extractor fan Toothbrush/mug and towel holders Mirror  STARBOARD 

GUEST CABIN Two single berths Bedside locker Wardrobe with shelf Mirror Storage locker Downlighters and individual berth lights  

OPTIONAL CREW CABIN One single berth Storage space Individual berth light Bathroom/WC: Wash basin Mirror  

POWER AND DRIVE SYSTEMS 4-bladed propellers in nickel aluminium bronze Bow thruster (125kgf) with dual-station controls Engine room lighting Lockable access hatch to engine room Power-assisted hydraulic steering system Trim tabs with indicator Electronic engine and gear shift controls Engine room extractor fans with electronic time delay  

ELECTRICAL SYSTEMS 24 Volt: 4 x heavy-duty batteries for engine starting 4 x heavy-duty auxiliary batteries Battery link facility with remote control at helm position Both battery banks are charged using a voltage sensitive relay that parallels both battery banks when a charging source is present 80-amp 24v battery charger Remote battery isolator control switches at main switch panel position 24v to 12v converters for certain navigation and radio circuits Circuit breakers on all circuits  220/240 Volt: 9.5kW generator in own sound shield with water-cooled and specially silenced exhaust Automatic fire extinguisher Shore support inlet in cockpit locker with storage for cable Polarity check system Generator/shore support changeover controls at main control panel Earth leakage safety trip Circuit breakers on all circuits Power points (240v) in: - owner’s stateroom - forward stateroom - galley (double) - saloon (2) Shaver points in all bathrooms  FUEL SYSTEM Twin fuel tanks (in NS8 marine grade alloy) with interconnection system giving 550 gallons (2500 litres) capacity Fuel fillers on port and starboard side decks High-capacity duplex fuel filters/ water traps

DISCLAIMER. The specifications displayed on this page are intended as a guide only. This boat is not available for sale, nor is it intended to be represented or marketed for sale in anyway by European Yacht Broker. All yacht specifications and informations are displayed in good faith but European Yacht Broker does not warrant or assume any legal liability or responsibility for the current accuracy, completeness, validity, or usefulness of any of the information and/or images displayed. This information is subject to change without prior notice and may not be current.  All trademarks, images and comments displayed on this page are the property of their respective owners.
