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GENERAL 
This technical report has as its object the description of the motorboat called "ADMIRAL", intended to be used as a restaurant, bar, venue for special events, music evenings, ceremonies, parties and evenings tema. The vessel is in possession of all the documents and certifications necessary to carry out the local navigation with authorization to carry a maximum of 250 passengers.
.

FEATURES OF THE SHIP

[image: image4.jpg]Name


: 
ADMIRAL
Leight


:
37,70 m
Large


: 
6,90m
Compartment Maritime  
:  
Genova 

Number 


  : 
8879
Service


: 
passengers transport
Navigation


: 
local
Year of costruction 

: 
1989
TSL


:
 237,29  tsl
TSN


: 
106,78 tsn
Material 
:
STEEL
Class 



: 
RINA
Passengers number 

: 
250
Bridges number

: 
2
CARAT
On the ship there are 2 bridges: 
• deck 
• upper deck 

On deck we find, from the stern, the following premises: 
1. covered porch, intended to accommodate guest accommodations 
2. corridor 
3. toilette men 
4. toilette women 
5. entrance hall 
6. local cuisine, as described later 
7. dining room, equipped with tables and chairs fixed 
8. Local men's locker room 
9. local women's locker room
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On the upper deck we have, from the stern: 

1. covered porch, intended to accommodate guest accommodations 
2. corridor 
3. multipurpose room, equipped with fixed side banks 
4. local bridge, no longer used for navigation, but can be visited by guests 
5.terrace smoking area
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All premises intended for the passage or to the stay of the guests have the bridges lined with non-slip material, washable, flame retardant, resistant to the corrosive action of disinfectants, pest resistant and not harmful.

ROUTES OF EXEMPT -TRAFFIC ROUTES, ACCESS DOORS AND STAIRS

The existing escape routes , meeting the requirements of regulation for maritime navigation safety , have been integrated with the opening of a new glimpse into the stern area to allow for a faster exodus from ship to dock in case of emergency.
All escape routes shall be indicated and illuminated .
Entrances, doors and stairs are available and meet the size requirements of the Regulations for Safety of Maritime Navigation . All the doors can be opened from both sides, and all the scales are equipped with railing and handrail regulations .

DESCRIPTION OF THE WAY TO EXEMPT :
The front door is located at the center of the left side of the ship size width 1.20 m - 2.00 m height . The access to the vessel is by means of a walkway in iron that connects directly to the ship at the wharf and the following dimensions width 95 cm, length 3.00 m . The walkway has a handrail , the transition zone has been treated with anti-slip material , the same is operated electronically .
In the bow area of the first deck of the ship , is located a closed room of administration ( 51 square meters ) which is used mainly in the winter season , the gateway has a size of 1 m wide and 2 m in height.
In the aft area of the first bridge is located a veranda ( 53 MQ ) , used as a dose.
The two areas of administration are connected by atrium entry and a corridor having a width of m . And a length of 1.30 meters . 2.00.
The upper deck is by means of an internal staircase and an external staircase with a width of 90 cm. On the upper deck are located: a multipurpose room 51 square meters that will be 'used to dance for private parties, birthdays, anniversaries, with a capacity of 40-50 people or bar according to the needs of the moment. A veranda of 39 square meters, which is used for bar service in the spring and summer seasons. The two areas are connected by atrium of about 16 square meters. Access to the multi-purpose hall is through an opening of Mt. 1 of width. In the bow area is located the control room and additional veranda of 20 sqm, from which you can 'access to the lower deck in the middle of a scale of external service with a width of 90 cm. Such scale is connected with the porch the hall inside the 1 bridge, through the openings of about 70 cm.

All halls are closed vessel equipped with windows that open.
FIRE PROTECTION
The active and passive protection fire fighting is made in accordance with the provisions of the Rules of Safety of Navigation Maritime and terrestrial decided in agreement with the technical Italian Naval Register :
to maintain protection system of fixed CO2 fire-fighting machinery space
to maintain the allocation of mobile fire extinguishers provided for the ship in the year and that is no. 10 kg powder extinguishers from 6 - 6 5 kg CO2 extinguishers , despite considering them redundant for the type of service that will be done .
There are two pumps in service existing fire on board.


LOCAL LIGHTING AND ELECTRICAL
The ship is in possession of no. 2 electric generators . The ship is in possession of no. 2 electrical systems , an implant is used when the ship is at sea , and an implant is used when the vessel is stationary at the dock and can ' purchase electricity from the ground that will power distribution panel with circuit breaker differential general up to standard.
The emergency lighting of premises and escape routes in the event of a power failure will be guaranteed by n . 16 emergency lamps Beghelli resettlement .

ACCESS TO SHIP
Boarding and alighting on the dock, for both guests and staff , can ' be done through access located on the side of the left half-length , where the vessel is moored alongside , and that stern where the vessel is moored at the stern. The passage from the dock to the ship will be realized with the arrangement of the catwalk to satin fitted with handrail on both sides.
TOILETS AT THE FARM
The ship is equipped with two rooms intended for male and female toilets . The premises are equipped with WC , wash basin, soap dispenser , hand dryers and are located on the first deck.

TOILETS FOR STAFF
The ship is equipped with a toilet for staff with shower and washbasin 
STRIPPED FOR HOME OR CABIN CREW
These rooms can be used both as crew cabins or for both staff changing rooms , located in the bow of the ship deck 1 .
There are also n. 3 cabin crew .

KITCHEN
The local cuisine is intended to be used by the staff in charge .. The room is equipped with steel walls coated in stainless steel , the floor is made of fire retardant material washable . The furniture and equipment are existing with all stainless steel surfaces . The room is equipped with n . 2 windows fitted with insect mesh .
Antecedent to the kitchen area is located out kitchen .
In the rooms you will find:
1 . a cooking plate gas for heating or the completion of the cooking of dishes that require completion
2 . a refrigerator industrial type with external thermometer able to guarantee the perfect conservation of the foods
3 . a bench in stainless steel for the subdivision in a portion of the food
4 . two sinks in double bowl
5 . an oven with six trays for heating / cooking of packaged foods , frozen foods , pre-cooked or otherwise prepared at the headquarters of the catering.
6 . A deep fryer with two bowls for frying necessarily impromptu
7. N. 1 dishwasher for dishes 
8. N. 1 dishwasher for glasses 
9. N. 1 sink outside the kitchen 
10. N. 1 workbench stainless steel out kitchen 
11. N. 2 freezers places in the local galley 

WATER SUPPLY 
The water supply is from crates ship when the ship is at sea and on land where the vessel is moored at the dock fixed, it is understood that the company is in possession of a contactor specially installed directly on the dock that feeds all utilities,  for the electric energy from the ground. 

LIQUID WASTE DISPOSAL 
As for the liquid waste: 
The waste water from kitchen and toilet rooms are conveyed in a pumping station located in the interiors of the ship that is taken periodically from the companies' addettel. 

EMISSIONS 
  There are n. 2 hoods placed in such space are channeled outside.
N. 250 JACKET lifebuoys 
lifebuoys 
DSC VHF radio 
NAVTEX 
N. 2 SART 
N. 1 EPIRB 
PUBLIC ADDRESS 
SPEED 10 NODS 
N. 2 ENGINES 300 HP TOTAL MADE IN THE USSR IN 1989 (VERY GOOD QUALITY) LOW CONSUMPTION
END OF REPORT 
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