Main Specification

Type: Drop center boad ketch Construction: Alloy hull, deck &

superstructure - AG4MC

Registry: Southampton Flag: British

Classification:

Year: 1991 Last refit: Maintained by her

Captain

Builder: ALU MARINE under current

owner supervision - FRANCE

Model: JEROBOAM - Ketch

Designer: Harle & Mortain Interiors: ALU MARINE

subcontractors with

owner supervision

Location: France Asking Price: EUR 750,000 (VAT not

paid)

L.O.A.: 68' 88'' - 21 m

Beam: 18' 4'' - 5.5 m

Draught: Min 4' 25'' - 1.3 m

Max 10' 5'' - 3.2 m

Gross tonnage: 44.8

Net tonnage: 35 t - Lead ballast: 12 t

Engines: GM V8 turbo diesel - 250 HP - 8.2 L - 5,900 hrs

Propulsion: * Shaft drive with oil lubricated sterngland

* 4 x blade bronze propeller

* ENGINE CONSUMPTION:

>> 17 L per hour @ 10 knots

Generators: N° 1 KOHLER diesel generator with sound shield - 7Kva/1,500 RPM/50 Hz -

15,120 hrs

Electrical: * 220V/24V circuits

* 12V circuits for equipment

* Electric leak detector

* Automatic water level control & adjustment level of all service batteries

* Service batteries : 12 x 2V 750Amp (2006)

* Dedicated engine batteries : 4 x 6V, 225Amp (2007)

* Generator battery : 1 x 12V, 112Amp

* Battery charger 50 Amp/24V

* 300W converter

* 25 Amp shaftdrive alternator

* 60 Amp alternator: service batteries

* 45 Amp alternator: engine battery

Fuel capacity: 2,200 L

Fresh water: 3,200 L

Black water: 150 L - s.s. tank

Grey water: 300 L - s.s. tank

Maximum speed: 12

Cruising speed: 8

Range in Nm: 1,300 Nm @ cruising speed

Navigation & Comm.: NAVIGATION EQUIPMENT

------------------------------

* GPS FURUNO GP 31

* GPS GARMIN 45

* Radar 24 Miles FURUNO

* Automatic pilot ROBERTSON AP 45 (with jack L&S reconditioned 2006) ,

the pilot can be released and is not interfaced with any other equipment

* Depth sounder VDO (+ repeater)

* Windvane Anemometre VDO (+ repeater)

* Magnetic compass RIVIERA (2 units)

* SSB Radio telephone 150W FURUNO (transmitter-receiver)

* VHF ICOME IC M45 Euro

Deck: GROUND TACKLE

--------------------

* Electric windlass LOFRANS 2,000 W with deck remote control & cockpit

control

* Double anchor bow roller

* Anchor CQR 70kg on 100 metres of chain 14 mm

* Anchor CQR 50kg on 60 metres of chain 14 mm

OTHER

--------

* Bathing ladder

* Bathing platform

* Teak cockpit table

* Cockpit sun awning

* Teak laid seats cockpit

* Sail locker

* Sun awnings

* Deck shower

* Cockpit cushions

* Sunbathing pads

Mechanical: * Twin steering wheels: cockpit + internal wheelhouse

* 17 x winchs BARIENT ST in bronze (8 winches in the cockpit)

Rig & Sails: GREEMENT KETCH

----------------------

* Main mast in aluminium SPARCRAFT, stepped to keel

* Mizzen mast SPARCRAFT

* ACMO s.s. deckware & oversized s.s. race tackles (genoa sheet)

* Twin s.s. roller furlers by RECKMAN: jib + genoa

* Self-tacking traveller jib

* Self tacking traveler: main boom

* Single backstay for main mast, Y backstay for mizzen mast

* 2 x set of spreaders (mizzen)

* 2 s set of spreaders (main mast)

* Spi pole in aluminium + jockey pool

* Kevlar sheets

* Moving runners

* Releasable forestay

>> Genoa, jib and runners control led back to cockpit

SAILS

------

* Genoa : 106 sq. m. CARAT - good condition

* Yankee (Solent) : 55 sq. m.

* Staysail : 22 sq. m. very good condition (2006)

* Main sail : 63 sq. m. semi full-batten - good condition (2003)

* Mizzen : 40 sq. m. CARAT in heavy Dacron (1991)

* Forestay sail : 72 sq. m.

* Spinnaker : 250 sq. m. - triradial cut with sock

* Stormsail : 35 sq. m.

* Mainsail and mizzen sails with new cover + lazy jack

* all sails come with a sail bag

Safety: * Complete offshore security equipment

* Life raft BOMBARD Offshore 8 persons - 8 years old - container

* 3 x bilge pumps MARINA ZZ 2,000 L/Hr,: all pumps switchable if needed

(sea water/fresh water)

* Securit glass 15/12mm for all the openings of the roof

* Engine room with automatic fire extinguisher system

Galley: GALLEY

---------

There is an independent galley area to port with a large s.s. worktop and

numerous lockers.

* Twin s.s. sinks

* Cooker with 3 gas burners + 1 electric plate 220V

* Air extractor

* S.S. gas oven

* Microwave oven

* S.S. refrigerator 200 L (cooling by sea water)

* S.S. freezer 100L (cooling by sea water)

* Crokery for 10 peoples

Other: * Towels & facecloths for 10 peoples

Sound & Video: * SONY HI FI system

* GRUNDIG multistandard TV screen + amplified antenna

* AKAI Multistandard video tape recorder

Tenders & Toys: * BOMBARD C3 (2006)

* Outboard engine YAMAHA 15HP (2006)

Accommodation:

Sleeps 10 in 3 double cabins and 1 crew cabin for 3

SALON

--------

The dining area to port can accomodate up to 8 peoples around a large wooden table.

The entertainment area comes with a TV, Hifi system, a 80L bar and a comfortable L shaped sofa.

* Triple opening deck hatches for natural ventilation and panoramic view thanks to her 10 large

portholes.

FORWARD CABIN

---------------------

* Double berth (140cm wide) + Pullman bed

* Hanging locker

* Stowage

>> ladder with deck access hatch

>> sail locker access

HEAD

------

* Electric WC Sanguineti

* Washbasin

* Shower

>> Access to sail locker

PORT & STARBOARD CABINS

----------------------------------

For each cabin,

* Double berth (140cm wide)

* Hanging locker

* Stowage

* Reading lights

* Opening deck hatch

HEAD (for each cabin)

---------------------------

* electric WC Sanguineti

* Washbasin

* Shower

AFT CREW QUARTER

------------------------

* Independent single berth to port with door

* Captain area with double bed to starboard

* Hanging closet

* Stowage

AFT HEAD

------------

* Electric WC Sanguineti

* Washbasin

* Shower

WATER SYSTEM

------------------

* WC SANGUINETI with DELOULE pump (sea and fresh water)

* Pressurised water circuit with DELOULE pumps (50Kg Compression at 6Kg, 2000L/h)

INSULATION

---------------

* STIRODUR closed cells foam insulation : 70mm under the deck, 120 mm for the hull

Cabins: 3 double + crew area for 3

Captain and Crew: 0

Comments:

JEROBOAM KETCH features a comfortable and airy interior thanks to her large roof and her warm elm wood

paneling. Unlike the other offshore cruisers, her protected cockpit & flat deck also offer generous

entertainment areas with sunbathing pads and cushions. As a drop center board shallow draft cruiser,

JEROBOAM KETCH allows access to protected remote anchorage's or to shallow water sailing areas with sandy

beach like the Bahamas...or Friesland in perfect security.

With her efficient deckware equipment and her seaworthy hull design by famous architect Philippe

Harle, JEROBOAM KETCH can be sailed single handed. Her single owner since new will be pleased to pass on his

10 years of successful sailing experience to the new owner.
Commenti:  

JEROBOAM KETCH rappresenta un comodo ed arioso interno grazie al suo grande tetto ed il suo caldo legno di olmo  

rivestendo di pannelli. Diversamente da altri incrociatori lungo la costa, la sua cabina di comando protetta & ponte piatto offre anche generoso  

aree di divertimento col prendendo il sole blocchi e cuscini. Come un asse di centro di goccia incrociatore di cambiale poco profondo,  

JEROBOAM KETCH permette accesso ad ancoraggio remoto protetto o abbassarsi aree di navigazione di acqua con sabbioso  

areni come la Bahamas... o Friesland in sicurezza perfetta.  

Con la sua attrezzatura di deckware efficiente ed il suo disegno di buccia idoneo alla navigazione di architetto famoso Philippe  

Harle, JEROBOAM KETCH può essere navigato singolo diede. Il suo solo proprietario fin da nuovo sarà lieto di passare sul suo  

10 anni di navigazione riuscita esperimentano al proprietario nuovo.  

