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SWAN 40 FRESS – HULL N°148

	Anno di costruzione 1999 – Designer: German Frers


SPECS
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	Lengh o.a. MT 12.67

Lenght waterline MT 9.88

Beam  MT 3.89
	Draft

Displacement

Ballast
	m       2,25  
Kg    10.000
Kg      3.170


HULL

The hull is built in "single skin" with hybrid fiber glass / aramid (Kevlar) reinforced with a polyester laminate. Structural bulkheads are marine plywood, waterproof (except for the bulkhead aft of the square that is in GRP sandwich).

Color: dark blue gelcoat NGA 7344

Sidebands: gelcoat NGA 2000 white

The central part of the pilot's seat and the top of the transom are integral and open becoming platform. Ladder is permanently attached to bathing platform.

The keel is elliptical in shape with bulb. The ballast is alloy of lead and antimony. The prisoners of the keel are made ​​of stainless steel with high-tensile washers welded to ensure the plug into the lead
	DECK


The bridge is in GRP, sandwich, with a core of foam PVC closed cell low density. Teck, 9 mm thick, glued with the "vacuum bagged" without screws. Strips along the rails for sheets Genoa

Falchetta anodized aluminum

System "floating Genoa" for the sheets Genoa

Stopper Lewmar Superlock

According passes chain on bow roller and bowsprit spinnaker mobile maneuver

Opening the stern pulpit

Pulpit with teak seat and opening

Opening the rail on the left.

Auxiliary engine bracket on the stern pulpit

Deck shower, hot and cold water
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WINCHES

Winches Lewmar Ocean Series WaveSpring: (A = Aluminium - ST = Self-Tailing -

E = Electric)

- 2 Lewmar 54 AEST electric winches for genoa sheets

- 2 sheets Spinnaker winches Lewmar 48 AST

- 2 x 44 AST on roof for halyards

- 1 x 44 AEST electric on roof halyard and reefing
ANCHOR AND MOORING

Electric anchor Lofrans Airon 1500 W - remote control with chain counter in the bow and cockpit - electric Quick windlass 500 W capstan, bow

Bruce Anchor - Chain, 50 m, diam. 10
INTERIORS

Square

Elk skin on the tie rods of the lands in square

Elk skin on the shaft in square

Aft cabin

2 portholes Goiot 34.14 between the cabin and the aft cockpit

kitchen

Salt water to sink, foot pump

Alpes Inox Gas, tilting, three burners, with oven and firm-pots. Safety device for flame control on each fire. Gas shut-off valve near the kitchen.

Remote control and gas leak detector installed near the gas cylinders, with control switch and visual alarm in the kitchen

Refrigerator Coolmatic powered by batteries or 220 V

Ice tray in the refrigerator.

2 Toilets

2 toilets Jabsco electric discharge through outlet to the sea. The WC Stern can even download in special stainless steel tank capacity of 60 liters, with suction nozzle on the bridge.

Salt water foot pump for both sinks

Electric pump for shower draining water tanks

Salt water to sink, foot pump

Coating in white GRP, up to the ceiling
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ENGINE

Nanni 4.150 HE, marine diesel engine, rated at 26.8 kW (35 hp) at 3,000 rpm mounted on flexible supports, mechanical inverter Hurth HBW 150 A, 2.63:1 reduction

About 1800 engine hours

Oil Capacity 240 liters in 2 tanks

Tank level indicators

Propeller: Volvo three-blade knives, clockwise, diameter 20 "(500 mm)

HYDRAULIC SYSTEM

Total capacity 425 liters (112.3 USg) in two stainless steel tanks located under the sofas of the square

Water tank level indicators

Digital meter water consumption BayFlow VMT

Watermaker Sea Fresh H204D, 63 l / hour, driven by the motor

Heating Eberspächer D5LC in all environments

Bilge pumps

2 Manual bilge pumps

Electric bilge pump, automatic control
ELECTRICAL SYSTEM 12 V

12 V 320 Ah Batteries Services

110 A alternator to charge the batteries and alternator service from 55 A to the starter battery

Engine start batteries 12 V 92 Ah

Command for parallel coupling of a starter battery with battery services

2 weatherproof sockets 12 V in the cockpit, including one high current inflation for tender

1 waterproof plug 12 V Dorade on a bow shaft

2 extra sockets 12 V to correspondence
Photovoltaic panel below the bow hatch

VHF / Windex and light on masthead

Foghorn, Aqua Signal, manual and automatic

Lights in closets 2 hangers

2 lights in saloon bulkhead Meta A0690

ELECTRICAL SYSTEM 220 V

Current attack on the quay 230 V 25 A

Rectifier / battery charger / inverter Mass 12/1200 VA, 50 VA

Rectifier / Inverter Victron Atlas 12/300 VA for TV

7 220 V sockets
TOOLS

Navigation equipment: Raymarine ST 60 + of 2011

1 analog repeater bolinometro 45 °, in the cockpit

1 analog repeater, 360, in the cockpit

3 Repeaters digital multifunction cockpit

All 5 tools near the main entrance hatch

2 digital repeaters at chart

1 analog repeater, 360 °, the correspondence

1 Checking autopilot, installed in the cockpit

Compass Suunto Suunto steering compass-bearing

2 VHF Shipmate RS 8300, one on the chart and one in the cockpit

Emergency VHF antenna installed on the stern pulpit and selective switch at chart

JRC GPS receiver d, d GPS Plotter Autohelm 200 and 600, Z331, installed at chart - plotter Raymarine E 90 NavPad in custody in the wheelhouse

Hydraulic Autopilot Autohelm 7000.

Radar Autohelm LCD, Z 335, and antenna onto the screen at chart table

TV 22 'with electric retractable system in saloon - digital terrestrial TV antenna

CD / DVD Player Philips

Radio / CD and Sony 10 CD charger with 2 speakers in cockpit and 2 in saloon

ARMAMENT

Tree in anodized aluminum alloy. Armament three sets of spreaders with flying and babystay

IG m 16.70 54.79 '

J m 4.85 15.91 '

P m 14.50 47.57 '

E m 5.05 16:57 '

Rail Harken System A and Battcar system for mainsail

Lazy jacks - Rail separate trysail

Removable forestay and the staysail halyard - two steps of tree

1 aluminum spinnaker Spinnaker pole - 1 Carbon fiber spinnaker pole - 1 Bouncer

Harken furling forestay

2 Navtec hydraulic tensioners, system 50, for the backstay split in two, and Boom Vang, Navtec System 50, with control unit on the pedestal of the steering wheel, towards the bow.
GENERAL EQUIPMENT

Mudflaps companionway entrance - Splash big cockpit

Cockpit cushions - removable table Teak cockpit - Awning complete

Covers for steering wheel and steering

SAFETY EQUIPMENT

Full safety equipment to RINA standards

Liferaft - lifebuoy automatic on stern pulpit

Cable connection for seat belts

SAILS

North Sails

Fully battened mainsail in Dacron

Furling genoa Dacron

Fully battened mainsail 3DL 2011

Furling genoa 3DL 2011

Genoa

Bow

Staysail

Trysail

Spinnaker

Gennaker

Copriranda
PRICE: EURO 270.000 VAT PAID + 5% BROKERAGE COMMISSION

INFORMAZIONI:
MASSIMO SANTIN: +39 348 2240195
I dati, indicati sono forniti dall’armatore si ritengono corretti ma non garantiti e non contrattuali. Commissioni (non incluse) di brokeraggio del 5% + iva da conteggiarsi sul prezzo di compravendita.
Venezia - Tel.+39.348.2240195-Fax +39.041.5206111
Marina di Punta Faro - 3/C, I-33054 Lignano Sabbiadoro (UD)
e-mail info@veniceyachts.com      www.veniceyachts.com
venice yachts


