General information
Brand/type          : Wauquiez Centurion 57
Name                    : Alice
Designer               : Berret – Racoupeau Yacht Design
Yard                      : Wauquiez, France
Year                      : September 2014
Hull number        : 57 #1
Construction        : Fibreglass
Length o.a.            : 17.70m
Length w.l.            : 15.36m
Beam                     : 4.95m
Draft                      : 2.50m
Weight                   : 22.500kg
Keel ballast           : 7.100kg (lead)
Water (L)              : 1.015L
Diesel (L)              : 615L
Location                : Port Camargue – France
VAT-status           : VAT not paid
Flag                       : French
Construction
· GRP/Balsa sandwich hull and deck built with the infusion process, ensuring an optimized resin/glass fibre ratio. Deck bonded to the hull via mechanical fasteners and polyurethane compound at bulwark level.
· Hull protected with a bisphenolic resin on outer layers of sandwich.
· Grey coloured hull (gelcoat).
· Composite hull structural grid, glassed and glued to the hull (acrylate urethane).
· Lead 2.50m deep draft keel, fastened with stainless steel bolts, nuts and counter plates.
· Rack & pinion transmission steering system with 2 steering wheels; composite rudder shaft.
· Teak side decks, coach house, cockpit seats and floor.
Deck fittings
· 2 x Harken 60.2STA electric Black Mainsheet winches (instead of standard 50.2STA manual).
· 2 x Harken 60.2STA electric Black Genoa winches.
· 2 x Harken 46.2STA electric halyard winches on cockpit coamings.
· 2 x Set of deck stoppers on cockpit coamings to port and starboard.
· 2 x Jib rails with ball bearing car/return to the cockpit.
· Ball bearing “Black magic” Harken blocks.
· Custom carbon steering wheels 1100 diameter.
· Cockpit cushions.
· Covers for steering wheels, winches and cockpit table in Cadet Grey fabric.
Deck equipment
· Tilting, teak slatted electric aft platform with remote control.
· Swimming ladder on aft platform.
· Cockpit shower with hot and cold water.
· Electric deck wash seawater pump.
· 1 x Shore power inlet on transom with cable.
· Fresh water inlet.
· Life raft storage in dedicated cockpit locker.
· 2 x Steering positions with compass, navigation panels, electronic engine control lever and engine panel to starboard steering position.
· 2 x Sheet lockers in front of steering stations with lids.
· Emergency tiller.
· Gas struts on cockpit lockers lids.
· 3 x Winch handle boxes.
· Cold moulded teak folding cockpit table with handrail.
· 2 x Opening portholes in cockpit for natural lighting and ventilation of the aft cabins.
· Spray hood (retractable in cabin top) with stainless steel structure built in grab rails.
· 8 x Stainless steel mooring cleats (foldable style).
· Stainless steel water and fuel intake fillers.
· Stainless steel stern pulpit with closing gate, life buoy support and flag pole support (flag pole included).
· “Open” type stainless steel pulpit.
· Double stainless steel lifelines.
· Stainless steel Stanchions with lateral opening gates.
· 2 x Deck lifelines with retractable attachment chain plates.
· 2 x Stainless steel handrails on cabin top.
· Manoeuvring lines and main halyard led under deck.
· Large flush stained PMMA lateral windows.
· 14 x Flush deck opening hatches, 8 x fixed portholes and 4 x opening ports.
· 1 x self-draining gas locker in port cockpit.
· Sail locker forward, stainless steel access steps, grating, sail storage, supports and electric bilge pump.
· Blue water security pack (including Zodiac 8-person life raft an 8 x inflating life jackets).
· Self-draining mooring locker with warp hook.
· Electric windlass 24V/2000W with 12mm gipsy.
· Delta anchor 32kg/70lbs with 50m/12mm chain and 50m/22mm warp.
· Stainless steel hull fitting anchor roller.
· Carbon in-hull retractable bowsprit.
· 6 x Mooring lines.
· 6 x Fenders with socks.
Spars and Rigging
· Keel stepped Sparcraft Performance mast painted black, with full batten mainsail pre-equipment with track/roller bearing cars. Sparcraft “Racing” beam.
· 3 Sets of aft swept spreaders.
· Anodised aluminium “Performance” boom painted black
· Hydraulic boomvang adjuster.
· Furlex headsail furler
· Rod rigging instead of standard Dyform: double backstay, forestay, lower, intermediate and upper shrouds.
· Hydraulic backstay adjuster.
· Hull side fitted upper and lower chain plates.
· Running rigging: Main and jib halyards, boom topping lift, main and jib sheets, jib furling line alongside bulwark.
Sails (made in France)
· Full 5 batten mainsail (Hydranet – triradial cut) 87sqm with sliding cars.
· Furling genoa (Hydranet – triradial cut) 65 sqm with UV-protection.
· Assymetrical spinnaker (Nylon) 198sqm with squeezer.
Electronic equipment
Chart table:
· 1 x B&G Multi Function Z12 EMEA.
· 1 x B&G Triton 42 repeater.
· 1 x Shipmate RS25 VHF with wire free handset.
· AIS transceiver and receiver.
Cockpit:
· Cockpit port: 1 x B&G Multi function screen Z8 EMEA, 2 x B&G Triton 41 repeaters with pilot command.
· Cockpit starboard: 1 x B&G Multi function screen Z8 EMEA, 2 x B&G Triton 41 repeaters + bow propeller command, B&G autopilot with Gyro compass RC42, Radar 4G BB, 3-Function captor: Speed/wind/depth, including Navionics XL9 chart.
· 4 x B&G Jumbo repeaters mounted on black powdered aluminium support.
Inside accommodation
The interior woodwork is built in teak and bees waxed.
The floorboard is made in Wengé. The deck is doubled with a GRP liner on which vinyl covered slats are fastened. The hull liner is made in teak and/or vinyl covered slats. For an outstanding comfort matrasses are made of memory of form foam. All berths are equipped with a slatted base and lee cloths and have cold moulded teak fiddles around the beddings.
Saloon
· One level saloon.
· Headroom 2.04m.
· Leather upholstery.
· Saloon entertainment pack with 40” flatscreen TV on lift system, with antenna and Blue-Ray player.
· BOSE stereo Radio/CD/DVD/MP3 sound system with USB inlet, bass subwoofer and loudspeakers in saloon and cockpit.
· Curtains/roller shades on all windows, hatches and portholes.
· Mosquito screens on all opening hatches.
· Webasto reversible (heat/cool) air-conditioning (water circuit & electric control).
· Stainless steel handrail fitted on the ceiling.
· U-shaped dinette to starboard with dining table on double stainless steel footing.
· Two extra seats for mail table.
· Storage under seats and backrests.
· Lounge chairs and navigation seat to port with storage behind backrests.
· Chart table with laptop dedicated space and storage.
· 24V/230V electric control panel.
Galley to port
· Headroom 2.02m
· Transversal galley both sides of the companionway.
· One lateral opening port (above stove).
· Synthetic marble double sink with hot/cold water mixer tap.
· Large working space in synthetic marble.
· Stainless steel gimballed 3-burner stove with oven.
· 230V microwave oven.
· Stainless steel 24V refrigerator 160L.
· 24V Negative cold icebox (160L).
· Wine cellar in galley to starboard.
· Washer/dryer 6kg (230V) in the galley.
· Numerous lockers and storage.
· Double refuse bin.
· 6 Sets dishwasher.
Forward master bedroom
· Headroom 2.02m and 1.86m under bridge deck.
· Master bedroom entertainment pack with 22” flatscreen TV, antenna and DVD-player.
· Hanging locker to port.
· Vanity to port behind hanging locker, with table, lighting, mirror and seats.
· Centreline bed 2.05m x 1.60m with drawers under.
· Bedside areas with book storage and reading lamp on each side of the bed.
· Wood slats base under bed (2 parts).
· Lee cloths.
· Lockers and storage alongside hull.
· Lockers and storage under companionway.
Bathroom for master bedroom
· Washbasin with pressurized hot and cold water.
· Lit cabinet with mirror.
· Stainless steel toilet accessories.
· Electric toilet with fresh water flushing.
· Independent shower compartment with mixer tap, grating and automatic draining pump. 
Aft guest bedrooms
Two double bedrooms
· Headroom 2.02m
· Double beds 2.05m x 1.40m.
· Hanging locker.
· Lockers under beds.
· Night shelf above bed head.
· Fixed hull portholes.
Two guest bathrooms
· Washbasin with hot and cold pressurized water.
· Lit cabinet with mirror.
· Marine porcelain toilet with sea and fresh water flushing system.
· Lateral opening port.
· Shower compartment (independent in starboard bathroom) with mixer tap, grating and automatic draining pump.
Engine equipment
· Yanmar 110hp engine / direct shaft transmission.
· Electronic engine control lever at steering positions.
· 3-Blade folding propeller.
· Rope cutter.
· 615L total fuel capacity (with decanting filter).
· 12V/85Ah engine start battery.
· Lit engine room with thermic/sound insulation.
· 24V/117kg vertically retractable bow thruster with independent battery.
Electrics
· 24V circuit with 8 x gel batteries (total capacity 540Ah).
· Insulated Onan generator 7kva (at 1.200 RPM) with 12v start battery.
· 24V/230V electric control panel at chart table.
· 2 x Mastervolt 60Ah battery chargers for 24V system.
· 1 x 25Ah battery charger for 12V batteries.
· Mastervolt batteries capacity control.
· Mastervolt inverter 24V/230V/2.500W.
· Recessed LED lights in ceiling.
· Switches with dimmers in saloon and at chart table.
· Reading lights at each bed, in the saloon and at the chart table.
· LED courtesy lights at floorboard level.
· LED navigation lights. 
Plumbing and fresh water
· 015L total water capacity with electric gauges.
· Pressurized fresh water inlet.
· 75L water heater working via engine or via 230V circuit.
· 24V – 36L/h pressure water pump with expansion tank.
· Automatic electric draining pumps in shower compartments.
· 2 x 80L holding tanks in head compartments.
Draining
· Self-draining cockpit, gas and anchor lockers.
· Automatic / control panel immerged electric bilge pump in sump at lowest point in hull.
· Double action manual bilge pump in cockpit.
Gas circuit
· Ventilated gas locker for two butane or propane containers.
· Solenoid safety valve.
 

