BENETTI  23 Displacement Motor Yacht  type « Navetta » 
Main characteristics  : 

Builder :  Benetti shipyard  Italy     Model & type :    Displacement Classic Benetti MY

Year :  1981  main refit  1997  San Diego USA  divers works  France 2002 -2003 -2004 .

L.O.A.   :  23 m   L.W.L.  :  20 m  Beam : 6 m    Draught :  3 m 

Displacement :  130 T    Gros tonnage :  107 T     Hull : steel    Superstructure : aluminium 

Fuel capacity :  20 000 liters      Fresh water capacity :   5 000 liters 

Engines & generators :
Main engines  : 2 x 170 Hp Gardner Sons Ltd  1981 rebuild totally in 1997 . 

Cruising speed :  10 konts at 1450 rpm  

Consumption :  34,5 liters / hour at 1200 rpm 

Range :  4 500 nm at 1200 rpm 

Engines controls :  cable  Morse 

Steering system : hydraulic 2 systems 

Gear boxes :  twin dics type 

Generators :  2 x 30 KW  Northern-Lights 1997 

                      1 x 5 kw on starboard engine 

Electronics and navigation equipment : 

Compass :  2 magnetic compass  SPERRY  

                   1 Gyro compass  ANSCHUTZ 

                   1 Gyro compass KVH US navy approved 

Radar :       1 Furuno 72 nm Color with all functions 

                   1 Furuno 48 nm 

Central Nav. : log / speedometer DATALINE 

Autopilot :   1 Robertson  AP 45 with repeater 

                     1 Sperry

Video plotter :  type Rob chart Robertson 

Vhf :   2  Icom 

           2  Sailor 

SSB  : 600 w Sailor 

Weather fax :  weather fax system Furuno 

Communication :  GSM unit  with 6 db antenna ( Us frequency )

                              Immarsat A phone & fax 

                              Immarsat  C  fax e weather fax 

Sounder :   3 units  one for 4000 feet 

Entertainment : 
Hi-Fi : Radio with CD player Philips

TV :  1  NTCS color  Tv  ( USA ) Sony 51 cms 

         1 Pal/secam  color TV  ( Europe ) Sony 51 cms 

         1 Portable  color Tv  Sony 

Systems : 
Stabilizers :   Vosper 

Air conditioned :  hot /cold  with thermostats Condaria  12 ventilo / convectors 

Water maker :  150 l/h  Desalator France 

Water heater : 1 central unit 

Air compressors :  Bauer for diving tanks + 1 to drive tools 

Fridges :  2 units  24 v/ 220 v  open compressor 

Tanks & bilges : 
Grey water tanks :  1 aft  250 l  - 1 front  250 l    manual / auto pumps 

Oil tanks :  1 new oil  125 l       1 used oil  125 l     transfer and discharge pump 

Bilge pumps :  220 v large pumps    - automatic  24 v pumps with alarms 

                        engine pumps direct on bilges  + manual bilges pumps + several units 

Electricity : 
Systems :  12 v  24 v  220 v      Converter system -  1700 amps  - 700 amps  

Batteries :  16 batteries  235 amp  ( 1997 ) 

Chargers :   1 x 150 amp  Caena        2 x 80 amp  Caena 

Deck equipment : 
Winches :  2 electric winches on aft deck 

Cameras :   camera with  monitoring system  : 2 x engine room  1 x aft deck  looking aft 

Teak :   complete teak deck  and side ways 

Fresh water :  fresh water connection for pipe    1 x front  1 x aft 

Canvas : 

Awings :  bimini for flying bridge 

Covers :  UV covers for each window 

Cushions :  cushions for each seat  4 x sun cushions on the roof    divers & numerous covers 

Mooring & security :
Anchors & chains :  2 x  Admiralty anchors      2 x  300 meters chains  galvanised new  diameter 14 mm 
Windlass hydraulic type with 2 pumps 

Ropes & fenders :  1 x 100 m rope  row type    4 x docklines   3 x Avon fenders  4 div. fenders 

Gangway : 1 x  aft med style    1 x from flybridge side  tidal harbours 

Tenders & engines : 1 x Avon with 4 hp Tohatsu     1 x  rigid Zodiac  40 hp  sussuki  

                                 1 electrical crane on fly 

Safety : 2 x 6 pers container liferafts    life jackets   all safety equipment for transatlantic cruise – 8 x fire extinguishers – engine room : Halon system . 

Accomodation : 
 Salon : a large salon with sofas in u shape  Dining area for 8/10  all furniture   bar  lockers  
Owners cabin : on main deck  dble bed   bathroom  with bath and  toilet 

Guest cabins :   lower deck front  2 identical cabins with 2 single beds & bathrooms

                         lower deck aft  : 1 large cabin with 2 single beds with bathroom 
Crew quarter  : 1 cabin  : 2 single beds  with bathroom 

                         1 cabin :  1 single bed  with bathroom 

                         1 laundry area with washing machine & dryer      1 fridge 24v /220 v 

Galley : 1 large sink C/H water – 1 oven – 1 Micro wave Europe 50 Hz – 1 Micro wave US type 60 Hz – 1 cooking plaques 4 x gaz & 2 electric – 1 dishwasher General Electric – 2 x fridges  24 v/220 v – 3 x fridges  24/220 v  located in food locker room -  all fridges controls –

Wheel house : all navigation instruments  witl all systems  Synoptic panels  etc ..

Flying bridge : acces from the wheel house with stairs case – navigation controls – seating area  with alarge table and teak deck – dinghy storage on cradles – electric crane Sanguinetti –

History : 

My Build by Benetti in 1981 – Actual owner purschased the yacht in 1991 – 

Made major refit in France then cruise for big and specific voyage –
This specific voyage took her from Europe to the west indies , up to America N.E. coast 

Up the Hudson Bay , then up to the Lawrence river .. back to the American East coast to
Patagonia , whre she crossed through the Magelan Passage to the Pacific Ocean …

She went to North to the Californian coast …

Stoped in 1997 for a major refit in yard San Diego  and came back to France after 

65 000 miles  in 1998 ..

That is the reason for she has been fitted with a bulb , carries  2 x 300 m chains  and big 

propellers protections ( 2 emergency shafts  and propellers in extra ) 

MY is now for sale , ready again for  high sea cruises …

