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M/Y   “MAMAI”
Builder                                                : Cantiere Navale di Lavagna

Type                                                    : ADMIRAL 35 

Construction material                       : wood  (hull : marine plywood internal and    

                                                                           Mahogany external)                                   

Year                                                     : 1981/rebuilt 2000

Superstructure                                   : new design (year 2000)  

Length O.A.                                        : 34,46 mt

Beam                                                    : 7.55 mt

Draft                                                    : 2.40 mt

Classification                                      :  R.I.Na – 100-A- 1.1 “Y” (due 2007)

All particulars are given in good faith and believed correct but they cannot be guaranteed.
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Gross tonnage                                     : 205 ton

Net tonnage                                         :    61 ton

Displacement                                       : 130 ton

Cruising speed                                       : about 24 kn

Maximum speed                                  : about 26 kn

Fuel consumption                               :  650 lt/hr

Flag                                                      : british

Asking price                                              : 3.500.000 EURO 

VAT                                                     : not due ( art. 60 del DLN 331 del 30/08/93)                                              

MACHINERY 
Engines                                                     : 3x1400 hp CAT type 3412E (year2000)

Trasmission                                              :  3x ZF 1950A   ratio 2,448:1 (year2000)

                                                                      With two hydraulic vickers pumps

                                                                      PVH 131C for bow thrusters and                

                                                                      stabilizers                              (year2000) Exhaust silencer                                      :  6x cowl  TXS 80 P                 (year 2000)

Exhaust pipes                               : moved from outside to inside           (year 2000) 

Propellers                                                 :  3x 5 blades-fixed pitch         (year 2000)

Propeller shafts                                       :  3x aquamet 17                       (year 2000)

All particulars are given in good faith and believed correct but they cannot be guaranteed.
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Seal shafts                           :  3x TAKAZAWA  tw  seal stern tsl type  (year 2000)
Generator                               : 1x40 kw ONAM

                                               1x19 EOFZ KOHLER                                 (year2003)

Bow Thruster                     :  hydro system  HBT-800 (70 hp)                (year 2000)

Stabilizer                             :  2x WESMAR R.S. 632                               (year 2000) 
Electricity                            : 380/220 volt , 24 volt

Inverter                               : 1x 9kw                                                           (year 2000)                

Fuel capacity                       : about 14000 lt

Fresh  water  capacity         : about  3500 lt 

Boiler                                                  : 2x SIGMAR 120 lt superinox     (year 2000)

Refrigeration compressor                : 2x 220 volt or 2x 24 volt               (year 2000)

Air conditioning                           : 2 set Cadenasso x 2 compressor (cold and warm)
Fresh water generator                      : 1x idromar  MC2 130 lt/hr           (year2004)

 N.B. Starting from year 2000  the yacht has been completely overhauled and refitted in most of her parts and equipments, in particular all pipes have been replaced, the electrical plant has been renewed, all pumps have been replaced.

All particulars are given in good faith and believed correct but they cannot be guaranteed.
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 NAVIGATION AND COMUNICATION EQUIPMENT 
Radar     : FURUNO 15-inch model FR-1500 MARK-3series          (year 2000)

Automatic Pilot   : 2x ROBERTSON autopilot AP8                          

Gyro Compass    : ROBERTSON SKR82                                           

Magnetic compass    : 2x FUSELLI

GPS                            : FURUNO navigator                                         (year 2000)                                                      
WIND                        :  B&G                                                                  (year 2000)

DEPTH              : 1X B&G  ,   1X color video sounder FCV-662      (year 2000)

VHF                           : FURUNO FM 8500                                           (year 2000)

Electronic charts      :  NAVIONICS  GEONAV  11 SUN                  (year 2000)

Television                  :  SEATEL model  TAC-92                                (year 2000)

TENDERS AND DECK EQUIPMENT

Tender                                 :1xNOVAMARINE RH 450 jet d with 1xYANMAR   

                                                Diesel 125 HP                                               (year2000)     

Tender crane                      : 1X about 1000 kg electric/ydraulic            (year2000)

Anchor Windlass                : 2x SANGUINETI electric                 

Anchor                                 : 2x HALL 240 kg                                         (year 2000)

All particulars are given in good faith and believed correct but they cannot be guaranteed.
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Capstain                              : 4x electric at aft
Hydraulic Stern gangway : PIN-CRAFT(inox-teak) electric/hydraulic(year2000)

DECKS

Lower deck

Three new cabins with private bathroom and separate shower for guests ( in the  ex crew area at fore). 
Four original staterooms with private bathroom and separate shower for guests.

Engine room.

Workshop.
Two new cabins with one bathroom and shower for crew.

Main deck

At fore a new large sun-deck with a trunk for tender, tender-crane and fenders,below.

A large dining-room.

A large galley.

A large store-room under bridge-deck.

A large lounge.

At aft a wide cockpit with a large hydraulic folding table for 12 guests with cushioned and sofa-type seats.
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Fly deck

Bridge-deck.

A second open bridge control.

A very large sun-deck equipped with cushioned seats and a dining table for 12/14 guests.

ACCOMODATION

Owner cabin                   : 1x king-size with separate walk-in dressing room

Guest cabins                   : 1x twins VIP 

                                         : 2x queen-size + a single bed

Guest cabins (ex crew area at fore)

                                         : 1x queen-size

                                         : 1x twin

                                         : 1x triple

N.B. all cabins are equipped with private bathroom and separate shower

Crew cabin                     : 2x twin + one bathroom with shower

All particulars are given in good faith and believed correct but they cannot be guaranteed.
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Main work done

YEAR 2000
New teak laid deck on fly deck.

New sun deck on main deck at fore with trunk for tender, tender crane and fenders, below.

New outside cushion seats. 

Hull and superstructure was totally sandblasted and repainted with allgrip paint.

All glass window was modified on main deck and upper deck.

Outside all glass window was lined of teak painted to copal.

 Four guest cabins was covered with tapestry.

All clothing of curtains,sofa and beds was replaced.

N° 6  round port-hole was replaced with N° 5  oval port-hole. 

The inside of the wale was lined of teak painted to copal.

All aluminium stanchions of the main deck were replaced with inox.

New  stern swimming platform (aluminium-teak) with new ladder. 

The cabins of the crew area at fore was modified for guests.

YEAR 2004

Rebuilt teak laid deck on main deck.

ALL PARTICULARS ARE BELIEVED TO BE CORRECT BUT NOT GUARANTEED
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