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Dimensions
LOA: 13.50 mt
Beam: 4.03 mt
D: 24,40 T


Engine

Engine  1x Volvo Penta D2-75S 75cv H:950  20.03.2015
Perfect conditions
 



Tanks

Fresh Water Tanks: (145 Gallons)
Fuel Tanks: (112 Gallons)
Holding Tanks: (31 Gallons)
Water Heater Capacity: (11 Gallons)




Accommodations

Number of cabins: 3
Number of bathrooms: 2



	
Sail Areas

· CRUISING 100 M²
· FURLING BOON MAIN SAIL  51 M²
· WORKING JIB 105% 46,4 M²
· GENOA 100 % (60 M² - 2014-
· GENNAKER (OPTION) 138 M²
· CODE 0 (OPTION) 87,5 M²  -2014-




	
Sailing

· Bow thruster
· Electric bow anchor with chain counter
· Winches, self tailing in stainless steel
· Cardan link rod steering
· Centaflex flexible coupling
· 3-bladed folding propeller
· Seldén rig
· Hydraulic integral backstay adjuster and rod kick with damper
· Internal main/jib halyards of Dyneema
· Headsail Furlex system
· Working jib
· Horn
· Compass
· Fully fuelled



	
Electrical-Electronics

· LED lights incl nav/anchor, cockpit, stern, boom and night lights
· Generator 3KW
· Battery charger  50a
· Inverter 2.5 kW/230 V
· Shorepower 230V
· Protection against lightning at shore power
· Isolation transformer and grounding plates for less corrosion
· Nº 6 Battery -2014-
· Autopilot E44G
· Radar AIS
· GPS Raymarine C120
· VHF Raymarine 240
· Wind Station  Raymarine ST60
· TV 28’ interface GPS
· DVD




	
Comfort

· Combi antenna RR/VHF, FM/AM, TV
· Sprayhood incl extension
· Skyscreen blinds in skylights
· AC Air heater incl cockpit outlet 
· Hot and cold water
· Transom shower (hot and cold water)
· Freshwater deck wash
· Toilet with electric flush
· Radio/CD-player with 4 speakers
· Corian top in galley
· Double sink in galley
· Gimballed stove with oven
· Combi oven hot air/micro/grill (230 V)
· Refrigerator, watercooled
· Freezer, watercooled
· Ebersparker hot air

	

Miscellaneous

· GRP hull with Divinycell sandwich core and
· Vinylester outer laminate
· Teak deck
· Teak pushpit seats
· High gloss varnished cockpit teak table and washboards
· Bow fitting incl twin roller
· Stainless steel bow protection rail
· Stainless steel windscreen
· Stainless steel cleats incl protection
· Two gateways in lifelines
· All tanks in stainless steel incl septic
· Life Saver rescue boy
· Automatic el. bilge pumps with alarm
· El. emergency pump 250 L/min
· Mooring ropes (4) and fenders (6)
· Antifouling -2014-




