JONGERT 16 S -  

          Main characteristics                                                                                                  Dimensions

NAME                                                                                      LENGTH O/A     17.30 MT   56’8’’

TYPE                       KETCH                                                    LENGTH W.L.    11,85 MT   38’9’’

SHIPYARD             JONGERT B.V                                        BEAM                  4,53   MT   14’9’

SERIES                    JONGERT 16 S                                       DRAUGHT          2,10   MT   6’9’’

ARCHITECT           DE VRIES LENTSCH                            DISPLACEMENT       TON 30

YEAR                       1977                                                        BALLAST                    TON 10

HULL MATERIAL  STEEL                                                    REFITT                 YEAR 2006

REGISTRY               ITALIAN                                                MAX. SPEED              9 KN

BERT                        LA SPEZIA                                            CRUISIN SPEED        7.5 KN

PRICE                       385.000,00 EUR                                     VAT                         EXEMPT

RING

          Ring                         Ketch

          Mast/s                      Rondal

          Reefing system/s     Slab reefing with lazi jaks for main and mizzen 

                                          Harken furling unit 2 for staysail  1998

                                          Harken furling unit 3 for jib 1998

SAILS

          Genoa                      Dacron

          Staysail                   North Sails,D’acron 1998

          Stormjib                  Dacron

          Yankee                    North sails,soft norlam,with foam fluff,80 m 2  1998

          Mps                         Zaoli 190 m2   2000

          Mainsail                  North sails,dacron fully  battened 52,3 m2  1998

          Mizzen                    North sails,dacron fully  battened  26  m2   1998

          Mizzen staysail       Zaoli 2001

          Winches                  2x Lewmar ST 55’’ 2 speeds

                                          2x Lewmar ST 48’’ 2 speeds

                                          2x Harken   ST 44’’ 2 speeds ( 1996 )




      2x Harken   ST 42”  2 speeds ( 1996)

MACHINERY  

          Engine                    Mercedes om 352,6 Cylinders

          HP  (kw)                 25  HP   (92) Kw

          Year                        1997

          Gear box                 Twindisc as 15

AUXILIARY EQUIPMENT 

          Bow thruster             Vetus 24 v,6 kw 1997

TANKAGE AND PERFORMANCE

          Fuel tank                     2800 l

          Fresh water tank         2200 l

          Waste water tank          500 l

          Total consumption           8 lt.   per hour

          Range approx.             2400 nm

ELECTRIC SISTEM

          Generator/s               Westerbeke 8 kw

          Inverter                      Prowatt 230 v/ 800 w

          Batteries                    6    X Sonnenschein gel batteris 12 v 230 A     2006

2 X fiamm 220 A  engine and bow thruster   2005

                                            1    X fiamm 80   A   generetor                         2005

 Batteri charter            Quich electronic 24 volt 80 A                           2000

 Shore Power              220 volt

NAVIGATION EQUPMENT

          Autopilot                    Furuno AP  330 and fluxgate compass  2000

          Sharp                          Quartermaster  B33

          Compass/gyro             Sestrel​ 

          Gps plotter                  Navionics Lcd   11 plus 1997

          Radar                          Furuno FS 1150 1997

          Weatherfax                 Furono fax 207 with active antenna and Navtex 

          Log                             B&G

          Depth sounder            Furuno Ls 6000 1997

          Wind speed                 B&G

          Direction                     B&G

          Rudder indicator         Yes

COMUNICATION

          Whf radio                     Skanti 3000 it 1997

          Ssb  radio                     Furuno Fs 1550, 150 W 1997

          Horn                             Hancofon automatic fog alarm

          Epirb                            Yes

          Intercom                       Yes

ENTERTAINMENT

           Tv/video                      Soniy Lcd 2004  17 ‘’

           Radio / HI FI               Kenwood 356 10 cd chargers. 10 loud speakers

DISTRIBUTION

            Owner                        Cabin 1- Berths 2 - Bathrooms 1,

            Guest                          Cabins 2 – Berths 4 – Bathrooms 2


Salon


Yes


Galley


Yes

AIR CONDITIONING


Heating

Webasto


Air conditioning
Condaria in salon ,  with reverse cycle


Ventilation

Webasto


Hot water heater
Electrical 1200 W

APPLIANCES


Refrigerator

Tadema  140  Lt.


Deep freezer

Tadema  120  Lt.


Microwave

Sharp


Stove


Roswell, electrical, 4 rings  ( 2003)


Safe


Yes

DECK EQUIPMENT


Bathing ladder
Yes


Deck shower

Yes


Awing


Yes


Cockpit cushions
Yes


Cockpit Cover

Yes


Anchor

2 x CQR


Windlass

Francis Marine Simpson Lawrence Type 1000


Deck wash system
Yes

TENDER AND WATER TOYS


Tender


Novamarine  Mod. RH 320


Engine ( tender )
Evinrude Hp 10  ( 2000 )

SAFETY


Life raft

Arimar 10 persons  ( 2005 )


Life jackets

Yes


Life belt

Yes


Bilge alarm

Yes


Fire-exinguishers
Yes

