HeySea 90’ Yacht

2 HeySea 90’ Principal Characteristics

Length overall: 27.43m（90’）（incl.pulpit）

Beam: 6.37m（20'11）

Depth: 4.07m（13'4）

Load Displacement： 76 ton

Navigation Area： along the coast

Engines： 2×CAT 1100hp

Max. Speed： 22 knots

Number of persons on

board： 20 persons

Range： 8 hours（200 miles）
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4 Specification

The data below refer to the standard version
1 Construction

Hand-laid FRP

Gel coat including stripes

Vinylester skin coat with

powderbound mat

Stitched multi-axial reinforced single

skin bottom

Balsa cored hull topsides

PVC foam cored deck and

superstructure

Hull stiffened with longitudinal

stringers supported by transverse

bulkheads and floors
2 Deck

Fittings all in stainless steel

Pulpit and cockpit rails

Stainless steel fendering with rubber

insert

Stainless steel bow roller with

anchor stop

Stainless steel anchor and 80m

chain

Electric winch and capstan with

deck, cockpit and flybridge

controls

Chain locker fender stowage

Curved direct glazed safety glass

windscreen

Pantograph windscreen wipers 24v

and washers

Fuel fillers port and starboard

Fresh-water filler

Ensign staff and socket

Fender tie bar under anchor locker

Lid
3 Bathing platform

Hot and cold swimming shower

Fresh-water marina connection

Dockside AC shore power

connection

Stainless steel swimming ladder

Lazarette stowage for fenders
4 Flybridge and helm position

Access hatch and stairs to saloon

and cockpit

Self draining

Acrylic deflecting spray screen

Compass

Steering indicator

Trim tab control Radar/Chartplotter

display

VHF handset (dual station)

Seating Table Instrument cover

Stainless steel guard rails and grab

rails

Glass holders

Wetbar with cold water

Cockpit speakers

Low-level flybridge lighting 24v

Lights under radar arch 24v
5 Aft cockpit

Teak-laid cockpit floor

Self draining

Stairs to flybridge

Stern seating

Side rope lockers

Stern safety doors

Engine room access hatch

Cockpit speakers

Overhead cockpit lights 24v

Low-level courtesy lights in aft

cockpit 24v

Low-level courtesy lights on side

decks 24v

6 Main helm console

Upholstered helm seat

Console with walnut fascia

Hydraulic power steering

Steering wheel

Radar/Chart plotter with GPS

Full analogue engine

instrumentation

Depth sounder

Rudder indicator

Fresh-water gauge Fuel gauge

VHF handset (dual station)

Compass

Horn Switch panels

Windscreen wipers with washers

Fire extinguisher

Side opening door to side deck

Chart stowage
7 Saloon

Large dining area in upper saloon

Air conditioning

Occasional seating in lower saloon

Plasma television (40”)

Hi-fi/DVD/CD surround system

Drinks cabinet

Stainless steel sliding cockpit doors

to aft cockpit

Halogen overhead lighting 24v

Low-level lights 24v

Generator controls

2 x double AC sockets

Choice of lacquered interior finishes

and veneers
8 Galley

Electric refrigerator and freezer

2-ring ceramic hob

Microwave/Oven

Stainless steel sink Hot and cold

water

Rubbish bin

8 place crockery set

8 place cutlery set

Cupboard and drawer, stowage

below

2 x double AC sockets

Fire extinguisher Hob extractor

Dishwasher

First aid kit
9 Master stateroom

Double berth

Storage beneath

Drawers in base-end

Dressing table with mirror and stool

Air conditioning

Halogen overhead lights 24v

2 x reading lights 24v

2 x opening portholes with mosquito

screens and curtains

4 x large fixed side windows

Double AC socket

Flatscreen television (26”)

DVD/CD player

Door to en suite bathroom

Door to en suite walk in wardrobe

Fitted carpet
10 Master en suite shower room

Vacuum toilet

Washbasin

Taps and accessories

Large shower

Extractor fan

Air conditioning outlet

Mirror

Toothbrush and glass holder

Towel ring and towels

Halogen overhead light 24v

Opening porthole with mosquito

screen and blind

Shaver socket 240/110v
11 Port guest cabin

2 x single berths
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Under berth stowage

Bedside unit with drawer

2 x reading lights 24v

Full hanging wardrobe

Air conditioning

Halogen overhead lights 24v

Opening porthole with mosquito

screen and curtains

Double AC socket
12 Port toilet/shower room

Vacuum toilet

Washbasin

Taps and accessories

Separate shower compartment

Extractor fan

Air conditioning outlet

Mirrored vanity unit

Shelved cupboard

Toothbrush and glass holder

Towel ring and towels

Halogen overhead light 24v

Opening porthole with mosquito

screen and blind

Shaver socket 240/110v
13 Starboard guest cabin

2 x single berths

Under berth stowage

Bedside unit with drawer

2 x reading lights 24v

Full hanging wardrobe

Air conditioning

Halogen overhead lights 24v

Opening porthole with mosquito

screen and curtains

Double AC socket

Door to en suite shower room

Overhead lockers

Flatscreen television (20”)
14 Starboard toilet/shower room

Vacuum toilet

Washbasin

Taps and accessories

Separate shower compartment

Extractor fan

Air conditioning outlet

Mirrored vanity unit

Shelved cupboard

Toothbrush and glassholder

Towel ring and towels

Halogen overhead light 24v

Opening porthole with mosquito

screen and blind

Shaver socket 240/110v
15 Forward guest stateroom

Double berth

Storage beneath

Drawers in base-end

Wardrobe

Dressing table with stool

Overhead lockers

Air conditioning

Flatscreen television (20”)

Halogen overhead lights 24v

2 x reading lights 24v

2 x opening portholes with mosquito

screens and curtains

Double AC socket

Door to en suite toilet/shower

Fitted carpet
16 Forward en suite shower room

Vacuum toilet

Washbasin

Taps and accessories

Separate shower compartment

Air conditioning outlet

Extractor fan

Mirrored vanity unit

Shelved cupboard

Toothbrush and glass holder

Towel ring and towels
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Halogen overhead light 24v

Opening porthole with mosquito

screen and blind

Shaver socket 240/110v
17 Crew cabin

Entrance door from the stern

Two berths

Wardrobe

Halogen overhead lighting 24v

Reading light 24v

AC socket
18 Crew toilet/shower

Toilet

Washbasin and shower

Mirrored vanity unit

Opening porthole with mosquito

screen and Venetian blind

Razor socket 240/110v
19 Engine compartment and

ancillaries

Soundproofing throughout engine

room

Fuel tanks with electric sending unit

Separate fuel filters/water

separators

Fire extinguisher

Engine room and forward bilge

flood alarms

2 x automatic bilge pumps

2 x automatic flood pumps

2 x extractor fans

Manual bilge pump
20 Electrical system

Slow speed generator with

underwater silent exhaust and

sound box

AC dockside connection

Galvanic isolator

24v and 12v DC electrical system

with full circuit breaker protection

4x engine batteries 24v circuit

2 x domestic batteries 24v circuit

1 x generator batteries 12v circuit

Alternator split charging system

Battery charger for 24v circuits

Battery charger for 12v circuits

AC sockets throughout the boat

24v hand light and cable
21 Underwater gear

4 blade bronze propellers

Bronze P-brackets

Stainless steel Temet 25 shafts

Dripless shaft logs with spare seals

High-performance bronze rudders

and struts

Seawater strainers

2 x CAT 1100HP

2 x generator 24kw

Full cathodic bonding system to

zinc anodes

Hydraulic bow thruster

Hydraulic stern thruster

Hydraulic trim tabs 24v
22 Systems

Hydraulic power steering engine

driven pump

24v vacuum toilet system

Toilet waste holding tank with

monitoring system

Aluminium fresh-water tank with

electric sending unit

24v fresh-water pressure system

Hot water tank

Washer/dryer in lower lobby
23 Miscellaneous

Toolkit

Boat hook

4 x mooring ropes

6 x fenders

Spare bulbs and fuses
