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	MORTOLA 

  YACHT  & SHIP BROKERS
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	Type  (Tipo)

Year   (anno costr.)

Builder  (Cantiere costruttore) 
Construction material (Materiale Costr.)

Length O.A.  (Lunghezza  f.t.)

Beam  (larghezza)

Draft (Pescaggio)

Machinery (Motori)

Max speed (Vel. Max)
Generator  (Gruppo elettrogeno)
Fuel capacity  (Capacità gasolio)

Fresh water (acqua dolce)

Accomodation (disp. Interni)

Flag (nazionalità)

Asking price   (Prezzo richiesto)
	Motor Sailor

1982/1983

Benetti 

Steel/Aluminium

16,25  mt

  4,70  mt

  2,35  mt

1 x175 Hp Volvo

9,2 Knots

Onan 13 kw 220 V
1.000 lt

2.400 lt

3 Guest cabins (2 x single, 1 x double) + 1 crew cabin

Italian

320.000,00 €


Via S. Michele di Pagana 32 - 16035  Rapallo  (GE) ITALY

Phone +39 0185 234 360  -  Fax +39 0185 234 352

e-mail :info@mortolabrokers.com
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NAVIGATION AND COMUNICATION EQUIPMENT (Apparati di navigazione e comunicazione)

Automatic Pilot (Pilota Automatico)  Neco / 2 position
Compass (Bussola) B & G Electric, Autopilot display
GPS : Philips + Geonav 
Radar : Furuno Range: 16 Nm
Radio VHF : Sailor
Radio SSB : Furuno

Echosounder (ecoscandaglio)  : B & G
Log : B & G

Chart plotter : Furuno

Wind indicator : B & G
MACHINERY & MECHANICAL EQUIPMENT
Engines: Type Volvo TMD 70C diesel  year  1983

  Engine hours: 3800 – date 2001

Gearboxes: Twin Disk 506

Bow thruster : Hydraulic 20 Hp/Kw

Air conditioning . Giusti

Heating : Giusti
GALLEY 

Refrigerator : 2 x make : Giusti

Deep freeze : 1 make: Giusti

Cooker : gas 4 flame

Oven : electric
Washer : Bosch

Dryer : Bosch

TV : Philips

Stereo
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RIGGING
Sails: 1 x Main

          1 x Genoa

          1 x Mizzen

Material : Dacron 1995

Sails area : 195 m2 (Main + Genoa)

Winches : 7 x Lewmar – selftail


   6 x Lewmar – hand – selftail


   1 x electric on stern

Masts Material : Aluminium

Furling sails : Genoa – electric
ELECTRIC

Batteries : Star set, 24 V Year 2001 3 x 120

                  Service set, 24 V Year 2000 4 x 200
Inverter : Landucci 24/220 V

Charger : Landucci

Shore power : AC 220 V – 50 Hz
TENDER AND DECK EQUIPMENT (Tender ed  attrezzatura di coperta)

Tender  : Eurovinil 1995 with Evinrude 15 hp outboard
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